**INVITATION FOR TENDERS (IFT)**



**OFFICE OF THE EXECUTIVE ENGINEER,**

**KNNL,GRBCC DIVISION No 3,GOKAK,TALUK: GOKAK,DISTRICT : BELAGAVI,STATE: KARNATAKA**

**PIN : 591307**

**Belagavi District : Ph: 08332-225213**

**Email : knnlgrbccd3.gokak@gmail.com**

**SHORT TERM DRAFT TENDER NOTIFICATION**

**(THROUGH "*e-Procurement*" ONLY)**

**TENDER NOTIFICATION NO. KNNL/GRBCC-3/GKK/DB/Tender/20 Arabhavi Tanks filling/2022-23/19**

Dt**: 04-03-2023**

On behalf of the Managing Director Karnataka Neeravari Nigama Limited, Bangalore, the Executive Engineer, KNNL, Karnataka Neeravari Nigama Limited, GRBCCDiv No-3, Gokak Taluk,, Belagavi, District : in Karnataka invites tenders on **LUMPSUM TURN-KEY and ITEM RATE** basis on e-procurement portal for the following work from KPWD Class-1 registration enrolled contractor.

The intending bidders shall submit bids as an individual / Joint Venture (JV) / along with Tie up with the pump manufacturer.

The two electronic document bid submission procedure as per Rule 28 of KTPP Act shall be followed.

The bidders are requested to submit their bids in two electronic document system including EMD in e-cash. The First Electronic Document (Technical Bid) should contain the documents as mentioned in Para 1.1 The Second Electronic Document shall contain the financial bid.

The First Electronic Document (Technical bid) will be opened first. Thereafter Second Electronic Document (financial bid) of only those bidders who have paid the requisite EMD and fulfil the conditions contained in Para.1.1 will be opened. The “contractor” herein means either an individual contractor or JV or a firm or a company.

The blank tender documents can be obtained through website [www.eproc.karnataka.gov.in](http://www.eproc.karnataka.gov.in) and can be submitted through electronic tender only.

**Table 1: The Details of work put to tender**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sl no** | **Name of work** | **Amount put to tender**  **(` Lakhs)** | **EMD**  **(` Lakhs)** | **Tender proc. fee (Non refundable)** | **Stiplated period for completion** | **Category of contractor Eligible** |
| 1 | 2 | 3 | 6 | 7 | 8 | 9 |
| 1 | “Survey, Investigation, Design, Supply, Installation, Testing and Commissioning of Lift System- Head Works consisting of construction of Intake Canal, Jack well cum pump house, Power Supply including terminal bay, 33 KV Electrical Substation, Transmission Line, Rising Main, Delivery Chamber & Gravity Distribution Network for filling of 20 Tanks of Arabhavi Constituency Of Belagavi District From Ghataprabha River (including 5 years Operation and maiantaince after successful completion) (Arabhavi TFS-Stage-1) on TURN KEY and ITEM RATE BASIS  PART A:Rs 948064800.56  **PART B: Rs** 591262909.08  **Total=Rs 1539327709.64** | Basic Cost+GST  **15393 + 2771 = Rs.18164.00 Lakhs** | The EMD of Rs.**1,81,64,000** shall be paid in full through e-payment or in two parts i.e,Part(1) Rs.**5,00,000/-** by e-payment Part (2) Rs.**1,76,64,000.00/-**  EMD shall be in the form Bank Guarantee in the prescribed format obtained from favour of Executive Engineer, KNNL GRBCC Division No.3 Gokak payable at Gokak | As specified in the e-procurement portal | 24 Months (including Monsoon) | KPWD Class-1 |

**Note:**

1. **The amount put to tender consists of the following.**

**a ) Turn key amount excluding GST Rs 153.93 Crores. The bidder should quote for this amount.**

**b) GST amount Rs. 27.71 Crores**

**2. The financial bid evaluation will be based on 1(a) above.**

**3. Quoted amount is exclusive of all deposits and supervision charges of ESCOMS. The amount will be paid by the Nigam.**

**PART A:** Part A Includes Survey, Investigation, Design, Supply, Installation, Testing and Commissioning of Lift System- Head Works consisting of construction of Intake Canal, Jack well cum pump house, Surge protection works, Power Supply including terminal bay, creation of 110kV/33kV bay with 1No.of 10MVA, 3-ph transformer and extension of existing 110kV bus at exisiting KPTCL Naganur substation, 33 KV Electrical Substation, Transmission Line, Rising Main , Pressure Distribution Network and all necessary Electormechanical works, Delivery Chamber for filling of 20 Tanks of Arabhavi Constituency Of Belagavi District From Ghataprabha River and Rejuvination of 7 nos of Tanks, Beautification for 1 tank, Approach/Linking/Concetivity road including CD works to Pump House and tanks (including 5 years Operation and maiantaince after successful completion).

**Part B:** Part B includes**:** Construction of Flood protection wall/retaining wall near sundholi village. The flood protection shall include construction of Gabion structure along the Flood protection wall/retaining wall (River side) with all necessary flood protection/erosion control work.

**CALENDAR OF EVENTS FOR THE TENDER PROCESS:-**

|  |  |  |
| --- | --- | --- |
| **No.** | **Calendar of Events** | **Date & Time** |
| a | The Contractor can have access to the e-tender document, i.e. the Tender schedules, bid documents and other documents in the web site http://eproc.karnataka.gov.in on payment of transaction fee (non-refundable) | **04.03.2023 onward up to 13.03.2023 up to 16.00 hours** |
| b | Last Date & Time for Tender Queries/Clarifications  [The queries if any are to be sent by the intending bidders through e-mail to the Executive Engineer (the e-mail id for sending queries is [knnlgrbccd3.gokak@gmail.com](mailto:knnlgrbccd3.gokak@gmail.com))] | **10.03.2023 at 16.00 hours.** |
| c | Pre–bid meeting will be held in the office of the Managing Director, Karnataka Neeravari Nigam Ltd, 4th floor, Coffee Board, No 1 Dr B.R Ambedkar veedhi, Bangalore. | **08-03-2023 at 11.30 hours.** |
| d | The Last date of Submission of completed Tender Documents through e-portal. | **13-03 -2023 upto 16:00 hours.** |
| e | First Electronic Document (Technical Bid (Cover –I)) will be opened in the Presence of the Bidders who wish to participate. | **14 -03 -2023 at 17.00 hours onwards.** |
| f | Second Electronic Document (financial Bid) of the successful bidders who qualify in the technical bid will be opened after approval to the technical bid from the competent authority. | After approval to the technical bid from the competent authority. |

## General

## Scope of Tender

The Executive Engineer, KNNL, GRBCC Div No-3, Gokak (Referred to as Employer in these documents) invites tenders following Two Cover tender procedure, from eligible Tenderers, for the construction of works (as defined in these documents and referred to as "the works") detailed in the Table given in the Invitation for Tenders (IFT). The Tenderers may submit tenders for any or all of the works detailed in the table given in IFT.

## Eligible Tenderers

Tenderers shall not be under a declaration of ineligibility for corrupt and fraudulent practices issued by the Government of Karnataka

## Qualification of the Tenderer:

* 1. All Tenderers shall provide the requested information accurately and sufficient detail in Section 3 : Qualification information
  2. To qualify for award of this contract, each Tenderer in its name should have in the last five years i.e. From 2017-18, 2018-19, 2019-20, 2020-21 & 2021-22.

## Qualification Criteria: (for Individual bidders/ Joint Venture Bidding).

|  |  |
| --- | --- |
| **(A)** | **Eligibility Criteria :** |
| 1 | The intending bidders should be a registered contractor enrolled in valid KPWD Class-I   1. The intending bidder can submit bids as an Individual/ Joint Venture bidder along with Tie –up of pump manufacturer. The Tie –up is to be formed prior to the bidding. In case of Joint Venture bidding, the lead partner should have at least 50% partnership |
| 2 | The requisite Earnest Money Deposit (EMD validity period is 180 days)  The EMD of Rs.**1,81,64,000** shall be paid in full through e-payment or in two parts i.e,Part(1) Rs.**5,00,000/-** by e-payment Part (2) Rs.**1,76,64,000.00/-**  EMD shall be in the form Bank Guarantee in the prescribed format obtained from favour of Executive Engineer, KNNL GRBCC Division No.3 Gokak payable at Gokak  (Using Credit Cards, Debit Cards, National electronic fund transfer & Over the counter) |
| 3 | Valid Employees Provident Fund Registration Certificate with latest Paid challen. |
| 4 | Valid GST Registration Certificate mandatory. |
| **Note:** | The Successful bidder shall furnish within 15 days from issue of letter of intent before entering in to agreement, a Copy of Income Tax returns filed mentioning PAN for the financial year 2021-22 (Assessment year 2022-23) prior to date of entering in to the agreement. Failing which the EMD amount will be forfeited and the tender will be rejected and the bidder shall be liable for subsequent penal action including black listing.  *The amount put to tender is exclusive of GST and the tenderer should quote without GST. However G.S.T will be paid at prevailing rate during billing.* |
| **(B)** | **Qualification Criteria :** |
| **a** | The intending bidder in his / its name should have in the last 5 years i.e., 2017-18 to 2021-22 achieved in at least 2 financial years, a minimum financial turnover of Rs.18164.00.00 Lakhs. (Rs. 18164.00Lakhs x 2 x 12 months /24 months). The turnover prior to FY 2021-22 will be updated to the Present Price Level (FY 2021-22) by giving weight age of 10% each year. Audited Profit and Loss account certified by a practicing Chartered Accountant bearing UDIN along with copy of Income Tax returns filed for the years indicated above should be furnished. |
| b | The intending bidder should have in last 5 years i.e. from 2017-18 to 2021-22, satisfactorily completed (not less than 90% of contract value) as a prime contractor, one similar work such as **LIS work** costing not less than Rs.**9082.00 Lakhs**.The work done certificate should be obtained duly signed from an officer not below the rank of Executive Engineer of the concerned Division and counter signed by the Superintending Engineer of the same circle or equivalent in case of other Government undertaking within India. The cost will be updated to the present value by giving a weight age of 10% for each year, if the work is completed prior to FY 2021-22.  Note-:1: Similar work means the work should comprise lift irrigation water supply scheme involving lift components such as intake Arrangement, Jackwell/sump, pump house, MS rising Main, Pressure/Gravity Distribution system, Electromechanical works, Delivery Mechanism (Delivery Chamber / Sump) with all arrangements  Note-:2: Work done certificate to be uploaded should have following information:   |  |  |  | | --- | --- | --- | | 1 | Date of Agreement | Date : \_\_\_\_\_\_ | | 2 | Agreement Period | \_\_\_\_\_\_\_\_\_ Months | | 3 | Contract / Agreement Value | Rs.\_\_\_\_\_lakhs | | 4 | Amount of work executed | Rs.\_\_\_\_\_lakhs | | 5 | % of Fin. Progress w.r.t. Contract value | \_\_\_\_\_\_\_\_\_% | | 6 | Date of completion of work | Date : \_\_\_\_\_ | | 7 | Copies of Last RA Bill / Final RA Bill shall be uploaded in e-procurement in support of work done certificate. | | |
| c | The intending bidder should have executed in any one year, the following minimum quantities of work (usually 80%of the peak annual rateof construction) during the last 5 years (i.e from 2017-18 to 2021-22). The necessary work done certificate issued by an officer not below the rank of Executive Engineer of the concerned Division and countersigned by the Superintending Engineer of the the same circle should be uploaded   |  |  |  | | --- | --- | --- | | Sl No | Item | Qty | | 1 | Earth work Excavation for Structures/pipeline including embankement | **1158083Cum** | | 2 | Reinforced Cement Concrete ( M15 grade and above) | **16424 Cum** | | 3 | Reinforcment Steel bars for RCC works | 753 MT | |
| d | The intending bidders shall submit bids as an individual bidder along with Tie–up of pump manufacturer. The Tie –up is to be formed prior to the bidding.  However, tenders from a Tie-up proposed in this bid, the bidder shall upload an agreement with only one pump manufactures on Rs. 200-00 stamp paper in the prescribed format which shall be concluded prior to bidding and enclosed to the bid document. For proof of the Tie up in the Technical bid in the prescribed format under section 2 of instruction to bidder (multiple tie–up not allowed). |
| e | Tendering by a joint venture is permissible subject to the following conditions:   * The joint venture shall be performed prior to the tendering and blank tender forms shall have been purchased by the joint venture itself * One of the partners of JV (Lead Partner) shall be duly authorized with a legally binding power of attorney to apply for tender forms and to sign the tender and to make further correspondences and deal with KNNL on behalf of JV * A contractor is not eligible to participate as partner of more than one JV * In case of JV all the partner are jointly and severally responsible for successful performance of the contract * The lead partner shall enter in to a joint venture agreement on Rs. 500 stamp Paper in the prescribed format which shall be concluded prior to bidding and enclosed to the bid document and submit along with the request for bid document. * The individual bidders of joint venture should be enrolled as KPWD Class-1 registration contractor separately. A copy of valid KPWD Class-1 registration certificate of individual bidders of joint venture should be uploaded.The lead partner should have at least 50% partnership. |
| f | The qualification criteria can be satisfied by individually or JV (adding collectively the credentials of all JV partners). The lead partners should have achieved at least 50% of prescribed annual turnover (Prequalification criteria), in any of the 2 financial years during the last 5 years (i.e., 2017-18 to 2021-22). Audited Profit and Loss account certified by a practicing Chartered Accountant along with copy of income Tax returns filed for the years indicated above should be furnished. |
| g | **The intending bidder should have laid and tested minimum quantity of MS Rising Pressure pipe system of the work with following diameter of pipes in any one financial year, during the last five financial years reckoned back from 2021-22.** Certificate should be obtained from an officer not below the rank of Executive Engineer of the concerned Division and countersigned by the SE of the concerned Circle or equivalent in case of other Govt. undertaking within India.  **MS pipe** with Inner diameter **300 mm** and above for length 2**0.00km** for MS Rising Pressure distribution system. |
| h | **The intending bidder (Individual/JV)/ Tie-up partner should have installed, tested & successfully commissioned at least 2 Nos. of VT Pumps with a capacity (Flow rate) not less than 0.110 Cumecs for each pump with head not less than 100.00 mtrs for each pump during the last 5 years (i.e from 2017-18 to 2021-22). The necessary work done certificate issued by an officer not below the rank of Executive Engineer of the concerned Division and countersigned by the Superintending Engineer of the the same circle should be uploaded** |
| i | **NOTES TO THE BIDDERS ON PQ:**   * The intending bidder should furnish data sheets for technical parameters of pumps, motor, transformers and other details sought under Section 14 Data sheets of the bid document. * The bid evaluation of electro-mechanical works will be done as per Section 8 Contract Data Clause No.20 bid evaluation factors. * Bids not satisfying minimum duty point parameters, efficiency parameters of pumps and motors and velocity parameters as specified in bid document shall be rejected. * No credit will be given during bid evaluation, if parameters higher than those specified in the Bid document- Section 8 – scope of work (in terms of duty point parameters, efficiency parameters of pumps and motors and velocity parameters) are offered by the bidder. * The successful bidder shall submit the tie-up agreement at the time of concluding the agreement for the work in the format prescribed in the bid document, failing which the EMD amount will be forfeited and contract will be rescinded at his risk and cost and liable for penal action including black listing. If one of the JV is pump manufacturer then tie-up with pump manufacturer is not necessary. * The tie-up arrangement will be generally permitted with the pump manufacturer whose data parameters are uploaded and in conformity with the details submitted in the data sheet of the bid document at the time of bidding. However, the successful bidder will be permitted to have tie-up agreement with other pump manufacturer provided his data parameters are unaltered with the uploaded parameters. * During technical evaluation KNNL find that any certification / information is false, such bidders will be disqualified and barred from participation in the bid their EMD will be forfeited. * If any bidder fails to satisfy the conditions mentioned above, such bids will be rejected. |
| j | Tenderers who meet the above specified minimum qualification criteria, will only be qualified, if their available tender capacity is more than the total tender value (Rs.Lakhs). The available tender Capacity will be calculated as under :  *Assessed available tender Capacity = (A×N×1.5 - B),*  *where,*  *A* = Maximum value of civil engineering works Executed in any one year during the last five years (updated to 2021-22 price level) taking into account the completed as well as works in progress.  *N* = Number of years prescribed for completion of the works for which tenders are invited.  *B* = Value, at 2021-22 price level, of existing commitments and on-going works to be completed during the next 24**months** (Period of completion of the works for which tenders are invited)  Note:-1: The statements showing the value of existing commitments and on-going works as well as the stipulated period of completion remaining for each of the works listed should be certified by Statutory Auditors of the Company or by the proprietor of the company through an affidavit.  Note:-2: Even though the Tenderers meet the above criteria they are subject to be disqualified if they have:  made misleading or false representation in the forms, statements and attachments submitted in proof of the qualification requirements  and / or  record of poor performance such as abandoning the works, not properly completing the contract, inordinate delays in completion, litigation history or financial failure etc,  and / or  Participated in the previous tender for the same work and had quoted unreasonably high tender prices and could not furnish rational justification.If the bidder / bidders have participated in more than one work, the available tender capacity will be assessed and number of works will be awarded as per his available bid capacity. |
| Note: | The bidder should furnish the details regarding qualification information in the prescribed format appended with bid document vide Section - 3 (i.e., Qualification information furnished by the bidder other than prescribed format is treated as non responsive). |

**3.3 Each Tenderer should further demonstrate:**

1. Availability by owning 50% of the required/specified flowing key and critical equipment for this work and the remaining 50% can be deployed on lease/hire basis for all works provided, the relevant documents (Commitment agreements etc.) for availability for the work are furnished (Documents to be scanned and enclosed)The intending bidder/firm/company/Joint venture should furnish details of ownership/ lease certificate of the following minimum requirement of machineries

| **Sl.No** | **Name** | **Own** | **Hire/Lease** |
| --- | --- | --- | --- |
| 1 | Excavator | 2 No. |  |
| 2 | Tipper | 4 Nos. |  |
| 3 | Concrete mixer | 2 Nos. |  |
| 4 | Vibratory Road Roller | 2 No. |  |
| 5 | Ultrasonic testing units |  | 2 No. |
| 6 | Radio graphic testing units |  | 2 No. |
| 7 | CRANE - Capacity 8 Tonnes and above |  | 2 No. |

1. In the case of the death of the contractor after executing the agreement / commencement of the work, his legal heir, if is an eligible registered contractor and is willing can execute and complete the work at the accepted tender rates irrespective of the cost of the work.
2. Necessary work experience certificate issued by the competent authority not below the rank of Executive Engineer, indicating the name/items of work executed, date of commencement, date of completion and the total cost of work executed shall be enclosed to the tender. Tenders without these details are liable for disqualification.
3. To qualify for a package of contracts made up of this and other contracts for which tenders are invited in this IFT, the Tenderer must demonstrate having experience and resources to meet the aggregate of the qualifying criteria for the individual contracts.

**3.3 (b) Each bidder should furnish liquid assets and/or availability of credit facilities of not less than Rs.3406.00 Lakhs from any Nationalised bank [Credit lines/letter of credit/certificates from banks for meeting the fund requirement etc. (Usually the equivalent of the estimated cash flow for 3 months in the peak construction period)]**

Format prescribed in respect of obtaining the Bank Certificate/Line of Credit:

**Bankers Certificate**

**This is to certify that M/s………… is a reputed company with a good financial status. If the contract for this work, namely………………………………(name of work) is awarded to the above firm, we shall be able to provide overdraft/credit facilities to the extent of …….. to meet the working capital requirements for executing the above work.**

**Sd/-**

**Name of the Bank, Senior Bank Manager**

**Address:………**

## Bid Capacity

Cover-II(Financial Bid ): shall containlump sum Turnkey amount with detailed break up of amount quoted.

The First Electronic Document (Technical bid) will be opened first and thereafter Second Electronic Document (financial bid) will be opened only of those bidders who qualify in the technical bid. In case the lowest bidder fails to produce the original documents for entering into an agreement or the original documents submitted does not match with the uploaded documents or found false ,then his bid is treated as non-responsive bid as per clause -26(4)of the KTPP rules & his name would be removed from the select list of KNNL enrolment and barred from participation in any of the tenders invited by the KNNL apart from forfeiting the EMD paid through E-cash.

## General Conditions:

1. The bid shall be technically evaluated based on the specifications indicated in Section-5 titled “Contract Data and Scope of work” in bid document.
2. The Bidder/JV partner/ Tie up partner shall not be under **Corporate Debt Restructuring** (CDR)/ Strategic Debt Restructuring (SDR) or Bureau of Industrial and Financial Reconstruction (BIFR) in the last 5 Years prior to bid submission date. In this regard, the Bidder shall submit along with Bid, a certificate from their Statutory Auditor with a declaration that, the Bidder is not under CDR/SDR or BIFR.
3. Bids not satisfying minimum duty point parameters, efficiency parameters of pumps and motors and velocity parameters as specified in bid document shall be rejected.
4. During technical evaluation, if the employer finds that any certificates / information furnished is false, such bidders will be disqualified and barred from participation in the bid.
5. If any bidder fails to satisfy the conditions mentioned above, such bids will be rejected and their financial bids will not be opened.
6. For laying M.S. pipe line the contractor shall engage only those agencies who have done similar job.
7. The bidder should enclose the detailed methodology of execution of the scheme as per the scope of work.
8. The Bidder shall be responsible for successful performance of the contract
9. For construction of Transmission line/Substation Works, the contractor shall engage only those agencies who are licensed to do the power line construction works in Karnataka. They should have constructed at least one similar single power line equal to 80% of the length of power line for the work tendered in a single contract. The details of the transmission line construction contractor with registration certificate and certificates of experience signed by an officer of not below the rank of Executive Engineer of KPTCL shall be submitted for KNNL’s verification post award of the work.
10. The Bidder to participate in the tender under single bid basis only. Any violation will attract disqualification of the bid.
11. The pump manufacturer shall not enter into Tie-up with more than one bidder.
12. The contractor/authorized signatory should attach his/her scanned signature to the Schedule-B before uploading and also submitting their tenders.
13. If any of the dates mentioned above happen to be a general holiday, the next working day holds good.
14. The work of the construction of transmission line should be got done through a Government Licensed, Super Grade Electrical contractor CEIG approved, who have the experience of carrying out such works.
15. The diameters of the rising main and thickness of the rising main shall not be less than the figures indicated in the enclosed schematic diagram. Further any discrepancies in the above shall not account to financial implications to the employer.
16. Further information can be had from the undersigned during office hours on telephone No: 08332-225213.
17. Conditional tenders are liable to be rejected. The officer competent to accept the tender shall have the right to reject any or all the tenders without assigning any reason whatsoever.
18. Corrigendum will be published in the web site/ newspapers of all modifications /corrections if any.
19. The intending bidders should note that, if any of lands either in part/ parts or in whole required for the work is not acquired by the Nigam, it shall be the responsibility of the bidder to take the possession of such land and start the work by obtaining consent of the land owners before commencement of work at no extra cost to the Nigam and no claim / delays whatsoever relating to on account of non-availability of land would be entertained.
20. The intending bidder should note that if they happen to be lowest bidder and awarded with the work, during the current financial year i.e. 2022-23, they should start only the Jack well work. Only after 50% completion of the Jack well work, the remaining works should be started by the agency.
21. If the percentage quoted by the contractor for the work is below ninety percent of the updated recast estimated amount put to tender, then the contractor shall furnish an “additional performance security” in the form of Bank Guarantee for an amount equivalent to the difference between the cost as per quoted percentage and 90% of the updated cost put to tender. In case of contractor quoting above 125% of updated cost put to tender, then the over and above 125% of the updated cost put to tender will be withheld during the progress of work. The additional performance will be released proportionately to the bill amount till the contractor achieves progress of the entire cost of the work as per agreement. The withheld amount in the later case will be released only after entire work contracted is fully completed and so certified by the Executive Engineer. (If BG submitted while issuing fresh BG or extending any existing BG, claim period of a minimum one year from the date of expiry of validity period of BG is to be specified invariably)
22. They should abide by the directions of Government towards recovery of 1% (or as modified by the Government from time to time) Cess from the contractor’s bill under the provisions of building and other constructions worker welfare cess Act 1996.
23. The intending bidders are advised to visit the site of work, make themselves familiar with local situation about the availability of construction materials, work men, land required for construction activities, etc and shall upload along with bid with details of references for visit of different parts of the scheme in the form of photographs of site.
24. The contractor is responsible for any damages due to natural calamity the government or Nigam will not give any compensation for until the completion of maintenance period.
25. The work proposed as per the scope of work is off-taking from the Ghaptaprabha river near Sundholi village in Gokak Taluka of Belagavi District. If any additions/alteration involved for during execution, it is the responsibility of the agency to deliver the goods as per contemplated scope of the work without causing any damages to existing infrastructure. If any damages occur during execution, the same shall be restored to the original condition at no extra cost.
26. The intending bidder/firm/company are advised to visit the work site before submission of the tenders.
27. The contractor should mention their recent correct portal address & mail address in declaration forms.
28. The tender processing charges paid by the bidder/firm/company are not refundable even if the tender is cancelled.
29. All materials like steel, cement, MS pipe etc., required for successful completion of the above work should be procured by the contractor only. No supply of any materials shall be made by KNNL.
30. The intending bidder should note that if they happen to be lowest bidder and awarded with the work, during the current financial year i.e. 2022-23.
31. The bidder/firm/company shall send the authorization letter for their representation duly attending their signature.
32. Maintenance period/Defect liability period for this work is **60 months** from the date of completion of work. (But for Aycut roads it is 12 months)
33. The bidder/firm/company shall adhere to accepted execution plan submitted by him under any circumstances without linking to the pending payment of the work & also land acquisition problems if any.
34. Typographical errors if any will not be the ground for any claims by the bidder/firm/company.
35. The amount put to tender is exclusive of GST. GST will be paid to the tendered amount separately as per prevailing rates. The contractor shall quote the rates excluding GST.
36. **Other terms and conditions as per Bid document & Tender Notification.**

**Sd/-**

**Executive Engineer**

**KNNL, GRBCC Division No 3, Gokak**

Copy submitted for kind information to:

1. Copy submitted to The Managing Director, Karnataka Neeravari Nigam Limited, 4th Floor. Coffee Board Building, Dr. B.R.AmbedkarVeedhi, Bangalore-560001/Walmi Campus, Belgaum Road, Belur, Dharwad for kind information and further need full.
2. Copy submitted to The Chief Engineer, KNNL, Irrigation North, Belagavi for information and further needful.
3. Copy submitted to The Inspector General of Police (Vigilance) Irrigation Department, BasavaBhavana, 4th Floor, Bangalore for favor of kind information.
4. Copy submitted to the C.A.O. Central Office of KNNL, Vijay Complex, Shrinagar Circle, Haliyal Road, Dharwad.
5. Copy submitted to The Superintending Engineer,KNNL,GRBCC Circle, Hidkaldam/ KNNL,GLBCC Circle, Jamakhandi / KNNL,R & R Circle, Athani for information and further needful
6. Copy forwarded to the Executive Engineers, KNNL, GRBCC Division No.2, Hidkal Dam / No.4. Chikkodi, / No.5, Koujalagi / MBC Division, Gaddanakeri for information and requested to publish in office notice board.
7. Copy to Assistant Executive Engineer, KNNL, GRBCC Sub Division no -5,6,7,8,Gokak.
8. Copy to the office Notice Board.
9. Copy to Executive Engineer’s Table / Audit officer’s Table.

**Sd/-**

**Executive Engineer**

**KNNL, GRBCC Division No 3, Gokak**